E614n19.wpd Feb 20, 2001    Wayne Faszer

Module Plane Foil Status Number Manufacture Date Optical Epoxy Comments

Dense Stack 200CO good T44 Sept 5/00 yes Appears to have scrape marks

                                                                                                    20DC failed T29 Aug 2/00 yes failed leak test Sept 7, passed

Sept 18

                                                                                                    22DC failed T42 Sept 5/00 yes failed leak test and reglued,

passed Nov 1

                                                                                                    17DC failed T33 Aug 2/00 yes failed leak test and reglued,

passed Oct 20

                                                                                                    16DC failed T39 Sept 5/00 yes failed leak test and reglued,

passed Nov 2

                                                                                                    21DC failed T41 Sept 5/00 yes failed leak test and reglued,

passed Nov 1

                                                                                                    18DC good T26 Aug 2/00 maybe little or no optical epoxy

But failed initial leak test

                                                                                                    15DC good T37 May /00 no passed initial leak test

                                                                                                    12DC good T22 Aug 2/00 no passed initial leak test

UV mod 3 Unknown good unknown unknown unknown

                                                                                                    9DC good T21 / 305 Aug 2/00 no                      Passed initial leak test

                                                                                                    7DC good unknown unknown unknown

Module Plane Foil Status Number Manufacture Date Optical Epoxy Comments

UV mod 4 202CO good T28 / 306 Jul 28/00 yes failed leak test and reglued

                                                                                                    10DC good T32 / 308 Jul 28/00 no passed initial leak test

                                                                                                    8DC good T25 / 307 Aug 2/00 no passed initial leak test

UV mod 5 Unknown good 12 Aug 20/99 unknown foil glued in

                                                                                                    6DC good 13 / 302 Aug 20/99 unknown

                                                                                                    5DC good 12 / 301 Aug 20/99 unknown removeable foil
yes the number 12 got used
twice

PPP 4 good unknown unknown probably glued in foil

                                                                                                    1DC good unknown unknown probably removeable foil

                                                                                                    2DC good unknown unknown probably glued in foil

                                                                                                    3DC good 9 May 5/99 probably foil glued in

                                                                                                    4DC good 13 Aug 20/99 probably glued in foil
likely some sealing with

       Optical epoxy but not the

Whole foil.

yes the number 13 got used
twice

Spare 23DC good T23 Aug 2/00 probably failed leak test and reglued