BEAM TUBE AND MOUNTING ASSEMBLY

G.M. Marshall TRIUMF

T WIST Collaboration Meeting Vancouver September 14, 2001

T WIST Beam Tube Extension

Status of the T WIST beam tube extension:

• design is completed.

• some drawings have been sent for manufacture.

Recent modifications to the design include:

• reduction of positron trigger scintillator diameter, to allow ±5 mm adjustment in x and y.

• lengthening of beam tube to reduce air gap to 55 mm. • allow small adjustment of z position of scintillators and beam tube.

Details of the geometry are now being included in the GEANT geometry definition.

The next three pages show side, top, and front views of the beam tube, scintillator support, and film degrader assemblies. The following two pages show the scintillator support installed in the yoke, and the final section of the beam tube with windows, respectively.