HV 2

HV 3

HV 1

3 mm 3 mm

HV 4

1 mm 0.5 mm

DME drift gas @ 20 torr

Aluminized mylar Field wire 50 - 100 mkm Sense wire 10 mkm

Aluminized mylar

20 mm

Fig. 1 Sketch of suggested time expansion chamber for muon track registration Drift region is between HV3 and HV4 planes.HV3 - HV4 = 80 V. Amplification region is between HV1 and HV3 . HV1 = HV3. Value ( HV2 - HV3 ) will be selected experimentally.